Windows Procedure

To calibrate, run the Windows executable WINCALIB.EXE. Locate the data files
of Appendix E and enter their locations into the interface at the appropriate
points.  CLMASC01.SUP and SUP01.CM will be specified on the "Dir/Files" page
as the "Met Data File" and "Actual Flow File", respectively.  The BNDCNDXX.SUP
file will be entered on the "Boundary" page, and the PARAM01.SUP file will
be specified on the "PARAMETERS 1" page.  

The configuration file (LBRM.CFG) must be specified on the "Dir/Files" page
as well as designating the working directory.  For simplicity it is suggested
that all of these files be located in the same directory, but that is not 
required.

Edit the boundary conditions and parameters as desired then click on the 
Start button.  To specify the starting parameter simply click on that
parameter on the grid on page "Parameters 1" prior to starting the 
calibration.

A log of the calibration process will be generated in the lower half of 
the interface which can be saved to a file and/or printed.


